[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - ON-VEHICLE SERVICE - SPEAKER TEST | PRINT PAGE / INDEX / PRIOR / NEXT

| SPEAKER TEST Enter the speaker test mode according to the following steps: Turn the Ignition switch to the "ACC" or "ON" position and switch off the radio and tape or CD player.
| Press the following buttons in that order within sixty seconds from step (1). Memory select "1" button "TUNE/SEEK (DOWN)" button "TUNE/SEEK (UP)" button Memory select "6" button
| Check that the speaker, which is displayed on the radio panel display, sounds (If the memory select "6" button is pressed, the speaker will be changed). If a button other than the memory select "6" button and "EJECT" button (tape or CD) is pressed, or the ignition switch is turned to "LOCK" (OFF) position, you will exit from the speaker test mode.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - ON-VEHICLE SERVICE - SPEAKER TEST | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation