[34] REAR SUSPENSION - - CONTROL LINK, UPPER ARM AND LOWER ARM - LOWER ARM BUSHING AND LOWER ARM PILLOW BALL BUSHING REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| LOWER ARM BUSHING AND LOWER ARM PILLOW BALL BUSHING REPLACEMENT
| Replace the lower arm bushing and lower arm pillow ball bushing as follows.
| LOWER ARM BUSHING REPLACEMENT CAUTION Because the outside of both edges of the bushing are different, be careful not to mistake the direction.
| Use following special tools to drive out and press fit the bushing. MB991447: Bushing Remover and Installer MB991448: Bushing Remover and Installer Base MB991449: Bushing Remover and Installer Supporter After press fitting, the space between the edges of the bushing outer sleeve and of the lower arm should be 1.5 mm.
| LOWER ARM PILLOW BALL BUSHING REPLACEMENT
| Use following special tools to drive out and press fit the bushing. MB990957: Lower Arm Bushing Remover and Installer MB990969: Guide MB990971: Base MB990996: Lower Arm Bushing Arbor After press fitting, the space between the edges of the bushing outer sleeve and of the lower arm should be 3 mm.

[34] REAR SUSPENSION - - CONTROL LINK, UPPER ARM AND LOWER ARM - LOWER ARM BUSHING AND LOWER ARM PILLOW BALL BUSHING REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation