[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A5. CHECK INTAKE AIR HOSE AND TURBOCHARGER OIL HOSE FOR DAMAGE | PRINT PAGE / INDEX / PRIOR / NEXT

| A5. CHECK INTAKE AIR HOSE AND TURBOCHARGER OIL HOSE FOR DAMAGE
| INTAKE AIR HOSES The air entered from outside the air cleaner element may make intake air dirty, resulting in engine power less than normal.
| Inspect the intake air hoses for cracks or damage.
| TURBOCHARGER OIL HOSES The oil leakage from oil hose may provide insufficient lubrication in the turbocharger, resulting in engine power less than normal. Inspect the turbocharger oil hoses for cracks or damage.

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS INSIDE THE ENGINE COMPARTMENT - A5. CHECK INTAKE AIR HOSE AND TURBOCHARGER OIL HOSE FOR DAMAGE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation