[15] INTAKE AND EXHAUST - - EXHAUST MANIFOLD - REMOVAL AND INSTALLATION <4G63-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

EXHAUST MANIFOLD

REMOVAL AND INSTALLATION <4G63-SOHC>
|  |  | Removal steps
--- | --- | --- | ---
<<A>> | >>A<< | 1. | Oxygen sensor
|  | 2. | Exhaust manifold cover
|  | 3. | Front exhaust pipe connection
|  | 4. | Gasket
|  | 5. | Exhaust manifold bracket
|  | 6. | Engine hanger
|  | 7. | Exhaust manifold
|  | 8. | Exhaust manifold gasket
| REMOVAL SERVICE POINT
| <<A>> OXYGEN SENSOR REMOVAL
| Use special tool oxygen sensor wrench (MD998770) to remove the oxygen sensor.
| INSTALLATION SERVICE POINT
| >>A<< OXYGEN SENSOR INSTALLATION
| Use special tool oxygen sensor wrench (MD998770) to install the oxygen sensor.

[15] INTAKE AND EXHAUST - - EXHAUST MANIFOLD - REMOVAL AND INSTALLATION <4G63-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation