[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - INSPECTION PROCEDURE P-8: When the power window main switch is operated, the switch signals are not received. <Vehicles for Argentina> | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE P-8: When the power window main switch is operated, the switch signals are not received. <Vehicles for Argentina>
| CAUTION Whenever the ECU is replaced, ensure that the input signal circuit is normal.
| COMMENTS ON TROUBLE SYMPTOM Input signal from the power window main switch is used in order to check the power window main switch and confirm how the system is communicating with the ETACS-ECU. If the communication line is defective, the power windows will not work normally.
| POSSIBLE CAUSES Malfunction of the power window main switch Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Check the operation by using the power window main switch. Check if each window can be operated by means of the power window main switch. Q: Can each power window be operated by means of the power window main switch? YES: Go to Step 2. NO: Go to Step 5.
| Step 2. Connector check: C-219 ETACS-ECU connector and E-05 power window main switch connector Q: Is the check result normal? YES: Go to Step 3. NO: Repair the defective connector.
| Step 3. Check the wiring harness between C-219 ETACS-ECU connector terminal No.59 and E-05 power window main switch connector terminal No.4. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-118, E-12 and joint connector C-02, and repair if necessary. Check the communication lines for open circuit. Q: Is the check result normal? YES: Go to Step 4. NO: Repair the wiring harness.
| Step 4. Replace the power window main switch, and then retest the system. Replace the power window main switch, and check that the power window main switch signal is received. Replace the power window main switch. Check that the power window main switch signal is received. Q: Is the check result normal? YES: The procedure is complete. NO: Replace the ETACS-ECU.
| Step 5. Connector check: E-05 power window main switch connector Q: Is the check result normal? YES: Go to Step 6. NO: Repair the defective connector.
| Step 6. Measure the voltage at the E-05 power window main switch connector. Remove the power window main switch, and measure at the wiring harness side. Voltage between E-05 power window main switch connector terminal No.6 and body earth OK: Battery positive voltage Q: Is the check result normal? YES: Go to Step 9. NO: Go to Step 7.
| Step 7. Connector check: C-208 power window relay connector Q: Is the check result normal? YES: Go to Step 8. NO: Repair the defective connector.
| Step 8. Check the wiring harness between C-208 power window relay connector terminal No.4 and E-05 power window main switch connector terminal No.6. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-118, E-12 and junction block connector C-203, and repair if necessary. Check the power supply line for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 9. Measure the resistance at the E-05 power window main switch connector. Remove the power window main switch, and measure at the wiring harness side. Continuity between E-05 power window main switch connector terminal No.2 and body earth OK: 2Ω or less Q: Is the check result normal? YES: Go to Step 11. NO: Go to Step 10.
| Step 10. Check the wiring harness between E-05 power window main switch connector terminal No.2 and body earth. NOTE: Prior to the wiring harness inspection, check intermediate connectors C-118 and E-12, and repair if necessary. Check the earth wires for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 11. Retest the system. Check that each switch signal is received by operating the power window main switch. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the power window main switch.

[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - INSPECTION PROCEDURE P-8: When the power window main switch is operated, the switch signals are not received. <Vehicles for Argentina> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation