[8] REFERENCE MATERIAL - - BOLTED PANEL FIT AND ADJUSTMENT - FUEL FILLER LID | PRINT PAGE / INDEX / PRIOR / NEXT

| FUEL FILLER LID
| FUEL FILLER LID FIT ADJUSTMENT
| If the levelling and clearance of the fuel filler lid is uneven, loosen the fuel filler lid mounting bolts, then move and adjust the fuel filler lid. Fuel filler lid mounting bolts tightening torque: 5.0 ± 1.0 N·m

[8] REFERENCE MATERIAL - - BOLTED PANEL FIT AND ADJUSTMENT - FUEL FILLER LID | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation