[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - TROUBLESHOOTING - SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

TROUBLESHOOTING

SYMPTOM CHART
Symptom | Inspection procedure No. | Reference page
--- | --- | ---
Speedometer does not work (the other meters work). <L.H. drive vehicles> | 1 |
Speedometer does not work (the other meters work). <R.H. drive vehicles for Hong Kong spec.> | 2 |
Speedometer does not work (the other meters work). <R.H. drive vehicles (Except for Hong Kong spec.)> | 3 |
Tachometer does not work (the other meters work). <L.H. drive vehicles> | 4 |
Tachometer does not work (the other meters work). <R.H. drive vehicles for Hong Kong spec.> | 5 |
Tachometer does not work (the other meters work). <R.H. drive vehicles (Except for Hong Kong spec.)> | 6 |
Fuel gauge does not work (the other meters work). <L.H. drive vehicles> | 7 |
Fuel gauge does not work (the other meters work). <R.H. drive vehicles for Hong Kong spec.> | 8 |
Fuel gauge does not work (the other meters work). <R.H. drive vehicles (Except for Hong Kong spec.)> | 9 |
Engine coolant temperature gauge does not work (the other meters work). | 10 |
Combination meters does not work (the instruments do not work). <L.H. drive vehicles> | 11 |
Combination meters does not work (the instruments do not work). <R.H. drive vehicles for Hong Kong spec.> | 12 |
Combination meters does not work (the instruments do not work). <R.H. drive vehicles (Except for Hong Kong spec.)> | 13 |

[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - TROUBLESHOOTING - SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation