[31] WHEEL AND TYRE - - ON-VEHICLE SERVICE - TYRE WEAR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| TYRE WEAR CHECK Measure the tread depth of the tyres. Minimum limit: 1.6 mm If the remaining tread depth is less than the minimum limit, replace the tyre. NOTE: When the tread depth of the tyres is reduced to 1.6 mm or less, wear indicators will appear.

[31] WHEEL AND TYRE - - ON-VEHICLE SERVICE - TYRE WEAR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation