[26] FRONT AXLE - - DRIVE SHAFT ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION Check the drive shaft for damage, bending or corrosion. Check the output shaft for damage, bending or corrosion. Check the drive shaft spline part for wear or damage. Check the output shaft spline part for wear or damage. Check the spider assembly for roller rotation, wear or corrosion. Check the groove inside PTJ case for wear or corrosion. Check the dynamic damper for damage or cracking. Check the boots for deterioration, damage or cracking.

[26] FRONT AXLE - - DRIVE SHAFT ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation