[26] FRONT AXLE - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIAL TOOLS
Tool | Number | Name | Use
--- | --- | --- | ---
| MB990767 | Front hub and flange yoke holder | Fixing of the hub
| MB991618 | Hub bolt remover | Removal of the hub bolt
| MB991897 | Ball joint remover | Knuckle and tie rod end ball joint disconnection NOTE: Steering linkage puller (MB990635 or MB991113)is also used to disconnect knuckle and tie rod end ball joint.
| MB990241 A: MB990242 B: MB990244 | Axle shaft puller A: Puller shaft B: Puller bar | Removal of the drive shaft
| MB991354 | Puller body
| MB991056 or MB991355 | Knuckle arm bridge | Removal of the hub Removal of the wheel bearing
| MB991721 | Sliding hammer | Removal of the output shaft <4WD>
| A: MB991017 B: MB990998 C: MB991000 | A, B: Front hub remover and installer C: Spacer | Removal of the hub Provisional holding of the wheel bearing Measurement of hub starting torque Measurement of wheel bearing axial play NOTE: MB991000, which belongs to MB990998, should be used as a spacer.
| MB990685 | Torque wrench | Measurement of hub starting torque
| MB990326 | Preload socket
| MB990810 | Side bearing puller | Removal of the centre bearing bracket Removal of the wheel bearing inner race (outside)
| MB991172 | Inner shaft installer base | Press-fitting of the inner shaft
| MB991248 or MB998801 | Inner shaft remover | Removal of the inner shaft
| MB991460 | Plug | Prevention of transmission fluid drain and of entry of foreign objects
| MB991561 | Boot band crimping tool | BJ boot (resin boot) band installation
| MB990925 | Bearing and oil seal installer set | Removal of the wheel bearing Removal and installation of the centre bearing Press-fitting of the dust seal outer, inner
| MB990890 | Rear suspension bushing base | Installation of the wheel bearing Press-fitting of the dust seal outer, inner
| MB990883 | Rear suspension bushing arbor | Installation of the wheel bearing
Tool | Type | Tool number | O D mm
--- | --- | --- | ---
| A | MB990926 | 39.0
MB990927 | 45.0
MB990928 | 49.5
MB990929 | 51.0
MB990930 | 54.0
MB990931 | 57.0
MB990932 | 61.0
MB990933 | 63.5
MB990934 | 67.5
MB990935 | 71.5
MB990936 | 75.5
MB990937 | 79.0
B | MB990938 | -
C | MB990939 | -

[26] FRONT AXLE - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation