[54A] CHASSIS ELECTRICAL - - FOG LAMP - FOG LAMP SWITCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

FOG LAMP SWITCH

REMOVAL AND INSTALLATION
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Instrument panel driver’s side garnish (Refer to GROUP 52A, Instrument panel assembly <L.H.drive vehicles> or <R.H.drive vehicles>)
|  | 2. | Meter bezel (Refer to GROUP 52A, Instrument panel assembly <L.H.drive vehicles> or <R.H.drive vehicles>)
|  | 3. | Fog lamp switch bracket
|  | 4. | Fog lamp switch (front and rear fog lamp switch) <Vehicles with rear fog lamp>
|  | 5. | Fog lamp switch (front fog lamp switch) <Vehicles without rear fog lamp>

[54A] CHASSIS ELECTRICAL - - FOG LAMP - FOG LAMP SWITCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation