[42] BODY - - FENDER - FENDER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

FENDER

REMOVAL AND INSTALLATION
Pre-removal and Post-installation Operation Front Bumper Removal and Installation (Refer to GROUP 51, Front Bumper <2000> or <2400>). Front Overfender Removal and Installation (Refer to GROUP 51, Overfender ) <Vehicles with Overfender>. Front Deck Garnish Removal and Installation (Refer to GROUP 51, Windshield Wiper ).
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Side sill garnish (Refer to GROUP 51, Garnish <Vehicles without Overfender> or <Vehicles with Overfender>.)
|  | 1. | Splash shield
<<A>> | >>A<< | 2. | Side turn signal lamp
|  | • | Headlamp assembly (Refer to GROUP 54A, Headlamp <2000> or <2400>.)
|  | 3. | Fender
| REMOVAL SERVICE POINT
| <<A>> SIDE TURN SIGNAL LAMP REMOVAL
| Use an appropriate tool such as special tool Ornament remover (MB990874) to pry out the tab from the fender, and remove the side turn signal lamp.
| INSTALLATION SERVICE POINT
| >>A<< SIDE TURN SIGNAL LAMP INSTALLATION
| Engage the hook with the fender panel, and install the side turn signal lamp.

[42] BODY - - FENDER - FENDER - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation