[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - ACCELERATOR CABLE AND PEDAL <4G63, 4G64, 4G69-L.H. DRIVE VEHICLES> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ACCELERATOR CABLE AND PEDAL <4G63, 4G64, 4G69-L.H. DRIVE VEHICLES>

REMOVAL AND INSTALLATION
Post-installation Operation Adjusting the Accelerator Cable (Refer to <4G63, 4G64> or <4G69-L.H. drive vehicles>).
|  |  | Accelerator cable assembly removal steps
--- | --- | --- | ---
|  | 1. | Inner cable connection (Accelerator pedal side)
|  | 2. | Inner cable connection (Throttle body side or accelerator pedal position sensor side)
|  | 3. | Accelerator cable assembly
|  | 4. | Accelerator cable bracket <4G69-L.H. drive vehicles>
|  | 5. | Holder <R.H. drive vehicles>
|  |  | Accelerator pedal assembly removal steps
|  | 1. | Inner cable connection (Accelerator pedal side)
|  | 6. | Accelerator pedal assembly
|  | 7. | Push-on spring nut
|  | 8. | Accelerator arm and accelerator pedal pad assembly
|  | 9. | Bushing
|  | 10. | Spring
|  | 11. | Stopper
|  | 12. | Accelerator pedal bracket
|  | 13. | Accelerator arm
| >>A<< | 14. | Accelerator pedal pad
|  | 15. | Accelerator pedal stopper
| INSTALLATION SERVICE POINT
| >>A<< ACCELERATOR PEDAL PAD INSTALLATION CAUTION To prevent damages to the Pedal Pad, warm the thumb area of the Pedal Pad with a dryer, etc. prior to assembling it. NOTE: If it is difficult to assemble, apply soapy water to the thumb area to enhance the assembling process.

[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - ACCELERATOR CABLE AND PEDAL <4G63, 4G64, 4G69-L.H. DRIVE VEHICLES> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation