[42] BODY - - DOOR - DOOR HANDLE AND LATCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| FRONT DOOR LOCK ACTUATOR CHECK
ACTUATOR OPERATION CHECK
LEVER POSITION | BATTERY CONNECTION | LEVER OPERATION
--- | --- | ---
At the "LOCK" position | Connect terminal No.4 and the negative battery terminal. Connect terminal No.6 and the positive battery terminal. | The lever moves from the "LOCK" position to the "UNLOCK" position.
At the "UNLOCK" position | Connect terminal No.6 and the negative battery terminal. Connect terminal No.4 and the positive battery terminal. | The lever moves from the "UNLOCK" position to the "LOCK" position.
ACTUATOR SWITCH CHECK <LEFT SIDE (LH DRIVE VEHICLES)>
LEVER POSITION | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
At the "LOCK" position | 1 - 2 | Less than 2 ohms
At the "UNLOCK" position | 1 - 3 | Less than 2 ohms
ACTUATOR SWITCH CHECK <RIGHT SIDE (RH DRIVE VEHICLES)>
LEVER POSITION | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
At the "LOCK" position | 2 - 3 | Less than 2 ohms
At the "UNLOCK" position | 1 - 3 | Less than 2 ohms
| REAR DOOR LOCK ACTUATOR CHECK
ACTUATOR OPERATION CHECK
LEVER POSITION | BATTERY CONNECTION | LEVER OPERATION
--- | --- | ---
At the "LOCK" position | Connect terminal No.4 and the negative battery terminal. Connect terminal No.6 and the positive battery terminal. | The lever moves from the "LOCK" position to the "UNLOCK" position.
At the "UNLOCK" position | Connect terminal No.6 and the negative battery terminal. Connect terminal No.4 and the positive battery terminal. | The lever moves from the "UNLOCK" position to the "LOCK" position.
| DOOR LOCK KEY CYLINDER SWITCH CHECK
<RIGHT SIDE (LH DRIVE VEHICLES)>
SWITCH POSITION | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
LOCK | 1 - 2 | Less than 2 ohms
NEUTRAL (OFF) | 1 - 2, 2 - 3 | Open circuit
UNLOCK | 2 - 3 | Less than 2 ohms
<LEFT SIDE (RH DRIVE VEHICLES)>
SWITCH POSITION | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
LOCK | 2 - 3 | Less than 2 ohms
NEUTRAL (OFF) | 1 - 2, 2 - 3 | Open circuit
UNLOCK | 1 - 2 | Less than 2 ohms

[42] BODY - - DOOR - DOOR HANDLE AND LATCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation