[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 11: Trouble related to the ETACS-ECU | PRINT PAGE / INDEX / PRIOR / NEXT

DIAGNOSTIC TROUBLE CODE PROCEDURES

Diagnosis code 11: Trouble related to the ETACS-ECU
| COMMENTS ON TROUBLE SYMPTOM The ETACS-ECU monitors the data, which the ECU itself sends. If errors occur consecutively 15 times (for 0.6 seconds), a diagnosis code will be set. Then, if the data does not contain any errors consecutively 15 times (for 0.6 seconds), the ECU will stop sending the diagnosis code.
| POSSIBLE CAUSE Malfunction of the ETACS-ECU
| DIAGNOSIS PROCEDURE
| Check whether the diagnosis code is reset. Erase the diagnosis code. Again check that diagnosis code No.11 is set. Q: Is diagnosis code No.11 set? YES: Replace the ETACS-ECU. NO: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ).

[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 11: Trouble related to the ETACS-ECU | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation