[55A] HEATER, AIR CONDITIONER AND VENTILATION - - HEATER CONTROL ASSEMBLY AND A/C SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| BLOWER SWITCH CONTINUITY CHECK
Switch position | Tester connection | Specified condition
--- | --- | ---
0 (OFF) | 1 - 2, 2 - 4, 2 - 5, 2 - 6 | Open circuit
1 (LO) | 1 - 2 | Less than 2 ohms
2 (ML) | 2 - 4 | Less than 2 ohms
3 (MH) | 2 - 5 | Less than 2 ohms
4 (HI) | 2 - 6 | Less than 2 ohms

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - HEATER CONTROL ASSEMBLY AND A/C SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation