[00] GENERAL - - VEHICLE IDENTIFICATION | PRINT PAGE / INDEX / PRIOR / NEXT

VEHICLE IDENTIFICATION
MODELS
FOR GENERAL EXPORT (Except for Hong Kong, Brunei, Singapore, Malaysia, Brazil, South Africa and Argentina)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU4W | XRHEZL/R | 4G64-SOHC (2,351 mL) | W4A42 <4WD, INVECS-II 4A/T> | MPI
CU5W | XRMYZL | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T>
XRHYZL
XRHJZL
(For Hong Kong, Brunei, Singapore, Malaysia)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU2W* | LRMER1D | 4G63-SOHC-Non-Turbo (1,997 mL) | F4A42 <2WD, INVECS-II 4A/T> | MPI
LYXFZR1D | 4G63-DOHC-Turbo (1,997 mL) | W5A51 <4WD, INVECS-II 5A/T>
CU5W* | XRHYZR1D | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T>
(For Brazil)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZL1F | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZL1F
(For South Africa)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZR6S | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZR6S
(For Argentina)
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRHYZL6A | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
FOR GCC
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZLW | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZLW
FOR NEW ZEALAND
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU2W* | LRMER1D | 4G63-SOHC-Non-Turbo (1,997 mL) | F4A42 <2WD, INVECS-II 4A/T> | MPI
LYXFZR1D | 4G63-DOHC-Turbo (1,997 mL) | W5A51 <4WD, INVECS-II 4A/T>
CU5W | XRMYZR8 | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T>
XRHYZR8
XRXYZR8
FOR AUSTRALIA
Model code | Engine model | Transmission model | Fuel supply system
--- | --- | --- | ---
CU5W | XRMYZR8 | 4G69-SOHC-MIVEC (2,378 mL) | W4A4B <4WD, INVECS-II 4A/T> | MPI
XRHYZR8
XRXYZR8
NOTE: * indicates the vehicles as "Hong Kong spec." in the running text.
MODEL CODE
No. | Items | Contents
--- | --- | ---
1 | Development | CU: MITSUBISHI AIRTREK/OUTLANDER
2 | Engine type | 2: 1,997 mL petrol engine 4: 2,351 mL petrol engine 5: 2,378 mL petrol engine
3 | Sort | W: Wagon
4 | Body style | L, X: 5-door hatchback
5 | Transmission type | R: 4-speed automatic transmission Y: 5-speed automatic transmission
6 | Trim level | H: GLS <Except for Hong Kong, Brunei, Singapore, Malaysia, New Zealand and Australia>, Sport gear <For Hong Kong, Brunei, Singapore, Malaysia>, XLS <For Australia and New Zealand> M: GLX <Except for Hong Kong, Brunei, Singapore, Malaysia, Australia and New Zealand>, 20V <For Hong Kong, Brunei, Singapore, Malaysia and New Zealand>, LS <For Australia and New Zealand> X: Turbo R <For Hong Kong, Brunei, Singapore, Malaysia and New Zealand(4G63)>, LIMITED <For Australia and New Zealand (4G69)>
7 | Specification engine feature | E: MPI-SOHC F: MPI-DOHC Y, J: MPI-SOHC MIVEC
8 | Special feature | None: 2WD Z: 4WD
9 | Steering wheel location | L: Left hand R: Right hand
10 | Destination | None: For General Export (Except for Hong Kong, Brunei, Singapore, Malaysia, Brazil, South Africa and Argentina) 1D: For Hong Kong, Brunei, Singapore, Malaysia and New Zealand (4G63) 1F: For Brazil 6S: For South Africa 6A: For Argentina W: For GCC 8: For Australia and New Zealand (4G69)

[00] GENERAL - - VEHICLE IDENTIFICATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation