[42] BODY - - SUNROOF ASSEMBLY - SUNROOF ASSEMBLY - DISASSEMBLY AND ASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

DISASSEMBLY AND ASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Deflector assembly
|  | • | Decoration cover (Refer to .)
|  | 2. | Adjusting plate
|  | 3. | Roof lid glass assembly
|  | 4. | Weatherstrip
| >>A<< | 5. | Weatherstrip inner
|  | 6. | Sunroof motor assembly
|  | 7. | Operating unit
|  | 8. | Sun shade assembly
|  | 9. | Lifter link
|  | 10. | Guide assembly
|  | 11. | Drip plate
|  | 12. | Seal tape
|  | 13. | Frame assembly
| INSTALLATION SERVICE POINT
| >>A<< WEATHERSTRIP INNER INSTALLATION Degrease the weatherstrip inner assembling surface of the roof lid glass side with unleaded gasoline.
| Assemble the weatherstrip inner in the location shown.

[42] BODY - - SUNROOF ASSEMBLY - SUNROOF ASSEMBLY - DISASSEMBLY AND ASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation