[31] WHEEL AND TYRE - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
ITEM | LIMIT
--- | ---
Tread depth of tyre mm | Minimum 1.6
Wheel runout <Aluminium wheel> | Radial runout mm | 1.0 or less
Lateral runout mm | 1.0 or less
Wheel runout <Steel wheel> | Radial runout mm | 1.2 or less
Lateral runout mm | 1.2 or less

[31] WHEEL AND TYRE - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation