[00] GENERAL - - TECHNICAL FEATURES - SERVICEABILITY AND RELIABILITY | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICEABILITY AND RELIABILITY
MAINTENANCE-FREE FEATURES Serpentine auxiliary belts and an auto-tensioner are adopted to eliminate the need for the adjustment of auxiliary belt tension.
ENHANCED DIAGNOSIS SYSTEM Diagnosis functions have been included for the following systems, so that it is possible to use the MUT-II/III to read the diagnosis codes and service data and to carry out actuator tests. In addition, it is also possible to read the diagnosis codes by the flashing of the warning lamp in some systems. MPI A/T 4ABS SRS air bag Smart Wiring System (SWS) Fully-automatic air conditioner
IMPROVED SERVICEABILITY AND HANDLING A part of the under cover is of a sliding structure to provide easy access for oil filter replacement. The speaker garnishes can be removed individually, which no longer requires the removal/installation of the door trims.

[00] GENERAL - - TECHNICAL FEATURES - SERVICEABILITY AND RELIABILITY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation