[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 5: The selector lever cannot be moved from the R to the P position. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 5: The selector lever cannot be moved from the R to the P position.
COMMENTS ON TROUBLE SYMPTOM The cause is probably a malfunction of the selector lever assembly or transmission control cable.
Possible causes Malfunction of selector lever assembly Malfunction of transmission control cable
DIAGNOSIS Check by referring to the possible causes.

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 5: The selector lever cannot be moved from the R to the P position. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation