[37] POWER STEERING - - STEERING WHEEL | PRINT PAGE / INDEX / PRIOR / NEXT

STEERING WHEEL The steering wheel is designed to improve operability, safety and maintainability and has the following features: The steering wheel is a genuine leather 3-spoke type with the steering shift switch on the upper surface of the spoke. <2000-DOHC> NOTE: The steering shift switch can be used in the AT sport mode. For steering shift switch, refer to GROUP 23, Steering Shift Switch . It has four spokes and comes in two types: with and without a (synthetic) leather cover. <2000-SOHC and 2400> It incorporates an airbag module to protect the driver in the event of a frontal collision. The airbag module is equipped with an inflator that does not contain sodium azide.

[37] POWER STEERING - - STEERING WHEEL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation