[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - ACTUATOR TEST REFERENCE TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

ACTUATOR TEST REFERENCE TABLE The MUT-II/III activates the following actuators for testing. NOTE: If the ABS-ECU runs down, actuator testing cannot be carried out. NOTE: Actuator testing is only possible when the vehicle is stationary.
| ACTUATOR TEST SPECIFICATIONS
No. | Item
--- | ---
01 | Solenoid valve for front-left wheel | Solenoid valves and pump motors in the hydraulic unit (simple inspection mode)
02 | Solenoid valve for front-right wheel
03 | Solenoid valve for rear-left wheel
04 | Solenoid valve for rear-right wheel

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - ACTUATOR TEST REFERENCE TABLE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation