[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 21: Cassette Tape can Not be Ejected. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 21: Cassette Tape can Not be Ejected.
| DIAGNOSIS PROCEDURE The problems covered here are all the result of the use of a bad tape (deformed or not properly tightened) or of a malfunction of the tape player itself. Malfunctions involving the tape becoming caught in the mechanism and ruining the case are also possible, and attempting to force the tape out of the player can cause damage to the mechanism. The player should be taken to a service dealer for repair.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 21: Cassette Tape can Not be Ejected. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation