[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 1: When the ignition key is at a position other than the LOCK (OFF) position, the selector lever can be moved from the P to the R position even though the brake pedal is not depressed. | PRINT PAGE / INDEX / PRIOR / NEXT

SYMPTOM PROCEDURES

INSPECTION PROCEDURE 1: When the ignition key is at a position other than the LOCK (OFF) position, the selector lever can be moved from the P to the R position even though the brake pedal is not depressed.
COMMENTS ON TROUBLE SYMPTOM The cause is probably a malfunction of the selector lever assembly lock cam or shift lock cable.
Possible causes Malfunction of lock cam Malfunction of shift lock cable
DIAGNOSIS Check by referring to the possible causes.

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 1: When the ignition key is at a position other than the LOCK (OFF) position, the selector lever can be moved from the P to the R position even though the brake pedal is not depressed. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation