[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - G-SENSOR <4WD> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

G-SENSOR <4WD>

REMOVAL AND INSTALLATION
<L.H. DRIVE VEHICLES> CAUTION Do not drop or apply a shock on the G-sensor.
Pre-removal and Post-installation Operation Rear Floor Console Assembly Removal and Installation (Refer to GROUP 52A, Floor Console Assembly .)
<R.H. DRIVE VEHICLES> CAUTION Do not drop or apply a shock on the G-sensor.
Pre-removal and Post-installation Operation Floor Console Assembly Removal and Installation (Refer to GROUP 52A, Floor Console Assembly .)

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - G-SENSOR <4WD> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation