[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - ACCELERATOR PEDAL POSITION SENSOR <4G69-L.H. DRIVE VEHICLES> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ACCELERATOR PEDAL POSITION SENSOR <4G69-L.H. DRIVE VEHICLES>

REMOVAL AND INSTALLATION
Post-installation Operation Adjusting the Accelerator Cable (Refer to ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Inner cable connection (Accelerator pedal position sensor side)
|  | 2. | Accelerator pedal position sensor connector
|  | 3. | Accelerator pedal position sensor assembly
|  | 4. | Accelerator pedal position sensor bracket
|  | 5. | Accelerator pedal position sensor bracket support

[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - ACCELERATOR PEDAL POSITION SENSOR <4G69-L.H. DRIVE VEHICLES> - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation