[11B] ENGINE OVERHAUL <4G6-SOHC> - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIAL TOOLS
Tool | Number | Name | Use
--- | --- | --- | ---
| MD998781 | Flywheel stopper | Retention of drive plate
| MD998778 | Crankshaft sprocket puller | Removal of crankshaft sprocket and crankshaft sprocket B
| MD998785 | Sprocket stopper | Retention of counterbalance shaft sprocket
| MB990767 | End yoke holder | Retention of camshaft sprocket (Use with MD998719.)
| MD998719 | Pulley holder pin | Retention of camshaft sprocket (Use with MD990767)
| MD998767 | Tension pulley socket wrench | Manipulation of tensioner pulley during adjustment of timing belt tension
| MD998443 | Lash adjuster holder | Retention of lash adjuster inside rocker arm when removing and installing rocker arm shaft assembly
| MD998713 | Camshaft oil seal installer | Installation of camshaft oil seal
| MD998442 | Air bleed wire | Air bleeding of lash adjuster
| MB991654 | Cylinder head bolt wrench | Removal and installation of cylinder head bolts
| MD998772 | Valve spring compressor | Compression of valve spring
| MD998774 | Valve stem seal installer | Installation of valve stem seal
| MD998727 | Oil pan remover | Removal of oil pan
| MD998162 | Plug wrench | Removal and installation of front case cap plug
| MD998783 | Plug wrench retainer | Removal and installation of front case cap plug (Use with MD998162)
| MD998371 | Silent shaft bearing puller | Removal of counterbalance shaft front bearing
| MD998372 | Silent shaft bearing puller | Removal of counterbalance shaft rear bearing
| MB991603 | Silent shaft bearing installer stopper | Guide and stopper for removal and press-fitting of counterbalance rear bearing
| MD998705 | Silent shaft bearing installer | Press-fitting of counterbalance front and rear bearings
| MD998375 | Crankshaft front oil seal installer | Installation of crankshaft front oil seal
| MD998285 | Crankshaft front oil seal guide | Guide for installation of crankshaft front oil seal
| MD998780 | Piston pin setting tool | Removal and press-fitting of piston pin
| MB990938 | Handle | Installation of crankshaft rear oil seal (Use with MD998776.)
| MD998776 | Crankshaft rear oil seal installer | Installation of crankshaft rear oil seal

[11B] ENGINE OVERHAUL <4G6-SOHC> - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation