[55B] AUTOMATIC AIR CONDITIONER - - ROOM TEMPERATURE SENSOR AND HEATER WATER TEMPERATURE SENSOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ROOM TEMPERATURE SENSOR AND HEATER WATER TEMPERATURE SENSOR

REMOVAL AND INSTALLATION
|  |  | Interior temperature sensor removal steps
--- | --- | --- | ---
|  | • | Instrument lower panel removal (Refer to GROUP 52A, Instrumental Panel ).
|  | 1. | Interior temperature sensor
|  |  | Heater water temperature sensor removal steps
|  | • | Driver's side foot duct removal (Refer to GROUP 55A, Ventilator ).
|  | 2. | Heater water temperature sensor clip
|  | 3. | Heater water temperature sensor

[55B] AUTOMATIC AIR CONDITIONER - - ROOM TEMPERATURE SENSOR AND HEATER WATER TEMPERATURE SENSOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation