[23A] AUTOMATIC TRANSMISSION (FF) - - SPECIAL TOOL(S) | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIAL TOOL(S)
Tools | No. | Name | Application
--- | --- | --- | ---
| MB991955 A: MB991824 B: MB991827 C: MB991910 D: MB991911 E: MB991825 F: MB991826 | MUT-III sub-assembly A: Vehicle Communication Interface (V. C. I.) B: MUT-III USB cable C: MUT-III main harness A (Vehicles with CAN communication system) D: MUT-III main harness B (Vehicles without CAN communication system) E: MUT-III measurement adapter F: MUT-III trigger harness | Checking A/T diagnosis trouble codes CAUTION If you connect MUT-III main harness A to a vehicle without CAN communication system to use the MUT-III, a pulse signal may interfere with the simulated vehicle speed lines, thus causing the MUT-III inoperative. Therefore, use the MUT-III main harness B (MB991911) instead.
| MB991502 | MUT-II sub assembly | Diagnosis code checking
| MB991529 | Diagnosis code checking harness
| MD991658 | Test harness | Voltage measurement
| MD998330 (including MD998331) | Oil pressure gauge (3.0 MPa) | Hydraulic pressure measurement
| MD998332 | Adapter | Oil pressure gauge connection
| MD998900
| MB990767 | End yoke holder | Fixing of the hub
| MB991897 | Ball joint remover | Knuckle and tie rod end ball joint disconnection NOTE: Steering linkage puller (MB990635 or MB991113)is also used to disconnect knuckle and tie rod end ball joint.
| MB990241 A:MB990242 B:MB990244 | Axle shaft puller A: Puller shaft B: Puller bar | Driveshaft removal Hub assembly removal
| A:MB991017 B:MB990998 C:MB991000 | A, B: Front hub remover and installer C: Spacer | Wheel bearing temporarily fixing NOTE: Use MB991000 (a part of MB990998 ) for spacer
| MB991721 | Sliding hammer | Output shaft removal
| MB991454 | Engine hanger balancer | When the engine hanger is used: Supporting the engine assembly during removal and installation of the transmission assembly NOTE: Special tool MB991454 is a part of engine hanger attachment set MB991453.
| MB991527 | Hanger
| MB991895 | Engine hanger
| MB991928 A: MB991929 B: MB991930 C: MB991931 D: MB991932 E: MB991933 F: MB991934 | Engine hanger A: Joint (50) × 2 B: Joint (90) × 2 C: Joint (140) × 2 D: Foot (standard) × 4 E: Foot (short) × 2 F: Chain and hook assembly

[23A] AUTOMATIC TRANSMISSION (FF) - - SPECIAL TOOL(S) | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation