[42] BODY - - DOOR - ON-VEHICLE SERVICE - POWER WINDOW CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| POWER WINDOW CHECK Check the system as described below. If the system does not work, carry out troubleshooting.Refer to GROUP 54B, Troubleshooting , refer to GROUP 54C, Troubleshooting , refer to GROUP 54D, Troubleshooting or refer to GROUP 54E, Troubleshooting . Operate the power window switch of each seat to check that the power window works. Turn on the power window lock switch of the power window main switch, and operate the front and rear passenger's power window sub switches to check that the power windows do not work. Turn on the power window lock switch of the power window main switch, and operate the power window main switch to check that each power window operates.

[42] BODY - - DOOR - ON-VEHICLE SERVICE - POWER WINDOW CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation