[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - ABS SENSOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

ABS SENSOR

REMOVAL AND INSTALLATION
Post-installation Operation ABS Sensor Output Voltage Measurement (Refer to .)
|  |  | Front ABS sensor removal steps
--- | --- | --- | ---
<<A>> |  | 1. | Front ABS sensor
|  | 2. | Front ABS rotor (Refer to GROUP 26, Driveshaft .)
|  |  | Rear ABS sensor removal steps
<<A>> |  | 3. | Rear ABS sensor
|  | 4. | Rear ABS rotor (Refer to GROUP 27A, Rear Hub Assembly <2WD> or refer to GROUP 27B, Rear Hub Assembly <4WD>.)
| REMOVAL SERVICE POINT
| <<A>> FRONT ABS SENSOR/REAR ABS SENSOR REMOVAL
| CAUTION Be careful when handling the projection at the tip of the ABS sensor and the toothed edge of the ABS rotor so as not to damage them by contacting other parts.

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - ABS SENSOR - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation