[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - LOW-REVERSE BRAKE - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

LOW-REVERSE BRAKE

DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
| >>A<< | 1. | D-ring
| >>A<< | 2. | D-ring
|  | 3. | Low-reverse brake piston
| REASSEMBLY SERVICE POINTS
| >>A<< D-RING INSTALLATION Apply ATF, blue petrolatum jelly or white Vaseline to the D-rings before installation, and handle them carefully not to damage them during installation.

[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - LOW-REVERSE BRAKE - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation