[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - DISCHARGING SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

DISCHARGING SYSTEM Use the refrigerant recovery unit to discharge refrigerant gas front the system. NOTE: Refer to the Refrigerant Recovery and Recycling Unit instruction Manual for operation of the unit.

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - DISCHARGING SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation