[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 4: The selector lever cannot be easily moved from the P to the R position. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 4: The selector lever cannot be easily moved from the P to the R position.
COMMENTS ON TROUBLE SYMPTOM The cause is probably a malfunction of the selector lever assembly, transmission control cable, shift lock cable, key interlock cable or ignition key cylinder lock bar.
Possible causes Malfunction of selector lever assembly Malfunction of transmission control cable Malfunction of shift lock cable Malfunction of key interlock cable Malfunction of lock bar
DIAGNOSIS Check by referring to the possible causes.

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T KEY INTERLOCK AND SHIFT LOCK MECHANISMS> - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 4: The selector lever cannot be easily moved from the P to the R position. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation