[42] BODY - - HOOD - ON-VEHICLE SERVICE - ADJUSTMENT OF HOOD HEIGHT | PRINT PAGE / INDEX / PRIOR / NEXT

| ADJUSTMENT OF HOOD HEIGHT
| Rotate the hood bumper by using the arrow mark on the hood bumper as a guide to adjust the hood height. If the hood bumper is rotated just one turn, the hood height changes by approximately 3 mm.

[42] BODY - - HOOD - ON-VEHICLE SERVICE - ADJUSTMENT OF HOOD HEIGHT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation