[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 12: Ever-Present Noise. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 12: Ever-Present Noise.
DIAGNOSIS PROCEDURE Noise is often created by the following factors, and often the radio is OK when it is checked individually. Traveling conditions of the vehicle Terrain of area traveled through Surrounding buildings Signal conditions Time period For this reason, if there are still problems with noise even after the measures described in inspection procedure 4 to 11 have been taken, get information on the factors listed above as well as determining whether the problem occurs with AM or FM, the station names, frequencies, etc. and contact the radio manufacturer's service centre.

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 12: Ever-Present Noise. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation