[11E] ENGINE MECHANICAL <4G69> - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIAL TOOLS
Tool | Number | Name | Use
--- | --- | --- | ---
| MB991502 | MUT-II sub assembly | Drive belt tension check Checking the ignition timing Checking the idle speed
| MB991955 A: MB991824 B: MB991827 C: MB991910 D: MB991911 E: MB991825 F: MB991826 | MUT-III sub assembly A: Vehicle communication interface (V.C.I.) B: MUT-III USB cable C: MUT-III main harness A (Vehicles with CAN communication system) D: MUT-III main harness B (Vehicles without CAN communication system) E: MUT-III measurement adapter F: MUT-III trigger harness | Drive belt tension check Checking the ignition timing Checking the idle speed CAUTION If you connect MUT-III main harness A to a vehicle without CAN communication system to use the MUT-III, a pulse signal may interfere with the simulated vehicle speed lines, thus causing the MUT-III inoperative. Therefore, use the MUT-III main harness B (MB991911) instead.
| MB991668 | Belt tension meter set | Drive belt tension check (used together with MUT-II or MUT-III)
| MB990767 | Front hub and flange yoke holder | Holding the camshaft sprocket
| MD998719 | Pin
| MD998772 | Valve spring compressor | Compressing valve spring
| MB991999 | Valve stem seal installer | Valve stem seal installation
| MD998713 | Camshaft oil seal installer | Camshaft oil seal installation
| MD998781 | Flywheel stopper | Supporting the A/T drive plate
| MB990938 | Installer bar | Crankshaft rear oil seal installation
| MD998776 | Crankshaft rear oil seal installer
| MD998285 | Crankshaft front oil seal guide | Crankshaft front oil seal installation
| MD998375 | Crankshaft front oil seal installer
| MD998738 | Adjusting bolt | Supporting the timing belt tensioner arm and timing belt tensioner adjuster
| MB991654 | Cylinder head bolt wrench (12) | Removal and installation of cylinder head bolt
| MB991367 | Special spanner | Holding the crankshaft camshaft drive sprocket
| MB991385 | Pin
| MD998767 | Tensioner wrench | Valve timing belt tension adjustment
| MB991454 | Engine hanger balancer | When the engine hanger is used: Supporting the engine assembly during removal and installation of the transmission assembly NOTE: Special tool MB991454 is a part of engine hanger attachment set MB991453.
| MB991527 | Hanger
| MB991895 | Engine hanger
| MB991928 A: MB991929 B: MB991930 C: MB991931 D: MB991932 E: MB991933 F: MB991934 | Engine hanger A: Joint (50) × 2 B: Joint (90) × 2 C: Joint (140) × 2 D: Foot (standard) × 4 E: Foot (short) × 2 F: Chain and hook assembly

[11E] ENGINE MECHANICAL <4G69> - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation