[00] GENERAL - - TECHNICAL FEATURES - TRANSMISSION | PRINT PAGE / INDEX / PRIOR / NEXT

TRANSMISSION
AUTOMATIC TRANSMISSION The W4A42 automatic transmission is adopted for the models equipped with 4G64 engine. The F4A42 and W5A51 automatic transmission is adopted for the models equipped with 4G63 engine. The W4A4B automatic transmission is adopted for the models equipped with 4G69 engine. The 4WD system uses the centre differential with limited slip device. The front differential is housed in the transfer (4WD). The centre differential is housed in the transmission in the place of the front differential for 2WD. A viscous coupling unit (VCU) is used for the centre differential limited slip device, and is located in the rear of the front differential. Incorporates the INVECS-II sports mode 4, 5-speed automatic transmission is adopted.

[00] GENERAL - - TECHNICAL FEATURES - TRANSMISSION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation