[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Item | Standard value
--- | ---
ABS sensor internal resistance kΩ | 1.24 - 1.64
G-sensor output voltage V <4WD> | Stationary vehicles | 2.4 - 2.6
Arrow facing downward | 3.4 - 3.6

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation