[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T> - INSPECTION CHART FOR DIAGNOSIS CODE <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION CHART FOR DIAGNOSIS CODE <4G69>
Diagnosis code No. | Diagnosis item | Reference page
--- | --- | ---
15 | A/T fluid temperature sensor system |
21 | Crank angle sensor system | Refer to GROUP 13C, Troubleshooting.
22 | Input shaft speed sensor system |
23 | Output shaft speed sensor system |
26 | Stop lamp switch system |
31 | LR solenoid valve system |
32 | UD solenoid valve system |
33 | 2ND solenoid valve system |
34 | OD solenoid valve system |
36 | DCC solenoid valve system |
41 | 1st gear ratio does not meet the specification |
42 | 2nd gear ratio does not meet the specification |
43 | 3rd gear ratio does not meet the specification |
44 | 4th gear ratio does not meet the specification |
46 | Reverse gear ratio does not meet the specification |
52 | DCC solenoid valve system |
54 | A/T control relay system |
56 | N range lamp system |

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T> - INSPECTION CHART FOR DIAGNOSIS CODE <4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation