[54A] CHASSIS ELECTRICAL - - IGNITION SWITCH - IMMOBILIZER SYSTEM DIAGNOSIS - DIAGNOSIS CODE CHART | PRINT PAGE / INDEX / PRIOR / NEXT

IMMOBILIZER SYSTEM DIAGNOSIS

DIAGNOSIS CODE CHART CAUTION During diagnosis, a diagnosis code associated with other system may be set when the ignition switch is turned on with connector(s) disconnected. On completion, confirm all systems for diagnosis code(s). If diagnosis code(s) are set, erase them all. Use the following chart to develop proper diagnostic strategy.
Diagnosis code No. | Diagnosis item | Reference page
--- | --- | ---
11 | Transponder communication system or radio interference of encrypted code | .
12 | Encrypted codes are not the same or are not registered | .

[54A] CHASSIS ELECTRICAL - - IGNITION SWITCH - IMMOBILIZER SYSTEM DIAGNOSIS - DIAGNOSIS CODE CHART | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation