[52A] INTERIOR - - REAR SEAT BELT - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

REAR SEAT BELT

REMOVAL AND INSTALLATION
<VEHICLES FOR SOUTH AFRICA, ARGENTINA AND AUSTRALIA>
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Rear seat cushion assembly (Refer to ).
|  | • | Rear seatback assembly (L.H.) (Refer to ).
|  | 1. | Inner seat belt
|  | 2. | Centre seat belt inner
|  | 3. | Centre seat belt garnish
|  | • | Quarter trim upper (Refer to ).
|  | 4. | Centre seat belt outer (Refer to ).
|  | 5. | Seat belt shoulder anchor bolt
|  | 6. | Seat belt lower anchor bolt
|  | 7. | Outer seat belt
<EXCEPT VEHICLES FOR SOUTH AFRICA, ARGENTINA AND AUSTRALIA>
|  |  | Removal steps
--- | --- | --- | ---
|  | • | Rear seat cushion assembly (Refer to ).
|  | 1. | Inner seat belt
|  | 2. | Centre seat belt
|  | • | Quarter trim lower (Refer to ).
|  | 3. | Seat belt shoulder anchor bolt
|  | 4. | Seat belt lower anchor bolt
|  | 5. | Outer seat belt

[52A] INTERIOR - - REAR SEAT BELT - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation