[27B] REAR AXLE <4WD> - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

SPECIAL TOOLS
Tool | Number | Name | Use
--- | --- | --- | ---
| MB991115 | Oil seal installer | Press-fitting of the differential carrier oil seal (Use together with MB990938)
| MB990767 | Front hub and flange yoke holder | Rear axle hub fixing
| MB990241 A: MB990242 B: MB990244 | Axle shaft puller A: Puller shaft B: Puller bar | Removal of the drive shaft
| MB991354 | Puller body
| A: MB991017 B: MB990998 C: MB991000 | A, B: Front hub remover and installer C: Spacer | Provisional holding of the wheel bearing Measurement of wheel bearing rotation starting torque Measurement of wheel bearing axial play NOTE: MB991000, which belongs to MB990998, should be used as a spacer.
| MB990883 | Rear suspension bushing arbor | Removal and installation of the differential support member bushing
| MB990984 | Mount bushing arbor
| MB990909 | Working base | Supporting of the differential carrier
| MB991116 | Working base adapter
| MB990810 | Side bearing puller | Removal of the side bearing inner race Removal of the companion flange
| MB990850 | End yoke holder | Companion flange fixing
| MB990339 | Bearing puller | Removal of drive pinion rear bearing inner race
| MB990374 | Pinion bearing remover
| MB990835 A: MB990836 B: MB990392 | Drive pinion setting gauge set A: Drive pinion gauge assembly B: Cylinder gauge | Adjustment of the drive pinion height
| MB990326 | Preload socket | Measurement of the wheel bearing rotation starting torque Measurement of the drive pinion turning torque
| MB990685 | Torque wrench
| MB990728 | Bearing installer | Press-fitting of the drive pinion rear bearing inner race
| MB990031 or MB990699 | Oil seal installer | Press-fitting of the drive pinion oil seal
| MB990925 A: MB990926 - MB990937 B: MB990938 C: MB990939 | Bearing and oil seal installer set A: Installer adapter B: Bar C: Brass bar | Press-fitting of differential carrier oil seal(Use together with MB991115) Inspection of final drive gear tooth contact Removal and installation of drive pinion front/rear bearing outer race For details of each installer, refer to GROUP 26 - Special Tools.

[27B] REAR AXLE <4WD> - - SPECIAL TOOLS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation