[1] PRE-DELIVERY INSPECTION - - BEFORE ROAD TEST - 22. AIR CONDITIONING, HEATER AND DEFROSTER SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

| 22. AIR CONDITIONING, HEATER AND DEFROSTER SYSTEM Check the systems for proper operation.
| Air conditioning Operate the air conditioning system. Operate the air conditioning light. Operate the control lever in all ranges. Operate the blower motor switch in all ranges.
| Heater and defroster After the engine has warmed up, turn on the heater. Operate the blower motor switch in all ranges. Move the control to "Defrost" position. A: From front and side defroster B: From centre ventilators C: From side ventilators D: From under the instrument panel E: From under the front seat (some models only)

[1] PRE-DELIVERY INSPECTION - - BEFORE ROAD TEST - 22. AIR CONDITIONING, HEATER AND DEFROSTER SYSTEM | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation