[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - SUNROOF TIMER FUNCTION CHECK <EXCEPT VEHICLES FOR ARGENTINA> | PRINT PAGE / INDEX / PRIOR / NEXT

| SUNROOF TIMER FUNCTION CHECK <EXCEPT VEHICLES FOR ARGENTINA> Keep the door closed, turn OFF the ignition switch and check to see if the sunroof operates for 30 seconds after that. If operations malfunction, perform troubleshooting. Refer to GROUP 54B, Troubleshooting , refer to GROUP 54C, Troubleshooting , refer to GROUP 54D, Troubleshooting or refer to GROUP 54E, Troubleshooting . NOTE: The adjustment function allows you to change the sunroof timer period from 30 seconds (initial setting) to 3, 10 minutes or "without function". Prior to the check, confirm which setting is activated <Vehicles for Hong Kong spec>.

[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - SUNROOF TIMER FUNCTION CHECK <EXCEPT VEHICLES FOR ARGENTINA> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation