[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - OPERATION AND FUNCTION QUICK-REFERENCE TABLE FOR INPUT SIGNAL INSPECTION PROCEDURES | PRINT PAGE / INDEX / PRIOR / NEXT

OPERATION AND FUNCTION QUICK-REFERENCE TABLE FOR INPUT SIGNAL INSPECTION PROCEDURES If troubles have occurred in the functions which use the SWS simultaneously, observe the table below to check input signals. (This table shows only the input signals which will cause troubles in at least two functions simultaneously).
Function | P-1 | P-2 | P-3 | P-4 | P-5 | P-6 | P-10 | P-12 | P-13 | P-14 | P-15 | P-16 | P-17
--- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | ---
Ignition key reminder function | - | × | - | × | - | - | × | - | - | - | - | - | -
Lamp reminder function | - | × | - | × | × | - | - | - | - | - | - | - | -
R (reverse) position warning | - | × | × | - | - | - | - | - | - | - | - | - | -
Door-ajar warning | - | - | - | - | - | - | - | - | × | - | × | - | -
Operating sound of turn-signal lamps | - | × | - | - | × | - | - | × | - | - | - | - | -
Downshift inhibitor buzzer | - | × | - | - | - | - | - | - | - | - | - | - | -
Control of central door locking | - | - | - | - | - | - | - | - | - | × | - | - | -
Key reminder function | - | - | - | × | - | - | × | - | - | × | - | - | -
Door locking released due to impact detection. | - | - | - | - | - | - | - | - | - | - | - | - | -
Keyless entry system | - | - | - | × | - | - | × | × | × | × | - | × | -
Keyless entry hazard warning lamp answerback | - | × | - | - | - | - | - | - | - | × | - | × | -
Multimode keyless entry system | - | - | - | - | - | - | - | - | - | - | - | × | -
Power window control | - | × | - | - | - | - | - | - | - | - | - | - | -
Power window timer | - | × | - | × | - | - | - | - | - | - | - | - | -
Sunroof control | - | - | - | × | - | - | - | - | - | - | - | - | -
Sunroof timer | - | × |  | × | - | - | - | - | - | - | - | - | -
Control of windshield wiper washer | × | - | - | - | - | × | - | - | - | - | × | - | -
Rear wiper washer control | × | - | × | - | - | × | - | - | - | - | - | - | -
Control of electric folding remote-controlled mirror | × | × | - | - | - | - | - | - | - | - | × | - | -
Ignition key cylinder illumination lamp function | - | × | - | × | - | - | × | - | - | - | - | - | ×
Headlamp control | - | - | - | - | × | - | - | - | - | - | - | - | -
Tail lamp control | - | - | - | - | × | - | - | - | - | - | - | - | -
Headlamp automatic shutdown | - | × | - | × | × | - | - | - | - | - | - | - | -
Fog lamp control | - | - | - | - | × | - | - | - | - | - | - | - | -
Turn-signal lamp control | - | × | - | - | × | - | - | - | - | - | - | - | -
Hazard warning lamp control | - | - | - | - | - | - | - | × | - | - | - | - | -
Dome lamp control | - | × | - | - | - | - | × | - | × | × | - | - | ×
Interior lamp automatic shutdown | × | - | - | - | - | - | - | - | - | - | - | - | ×
Door-ajar indicator lamp | - | - | - | × | - | - | - | - | × | - | - | - | ×
Security alarm | × | - | - | - | - | - | - | - | × | - | - | × | -

[54C] SMART WIRING SYSTEM (SWS) USING SWS MONITOR <Hong Kong spec.> - - OPERATION AND FUNCTION QUICK-REFERENCE TABLE FOR INPUT SIGNAL INSPECTION PROCEDURES | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation