[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 35: SRS-ECU Air Bag Condition Monitor Detects Deployed Air Bag | PRINT PAGE / INDEX / PRIOR / NEXT

Diagnosis code 35: SRS-ECU Air Bag Condition Monitor Detects Deployed Air Bag
DIAGNOSIS CODE SET CONDITIONS This diagnosis code is set after the air bag has deployed. If this diagnosis code is set before the air bag has deployed, the cause is probably a malfunction inside the SRS-ECU.
PROBABLE CAUSE Malfunction of the SRS-ECU
| DIAGNOSIS PROCEDURE Replace the SRS-ECU. (Refer to ).

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 35: SRS-ECU Air Bag Condition Monitor Detects Deployed Air Bag | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation