[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

ENGINE CONTROL

GENERAL INFORMATION
<4G63, 4G64, 4G69-L.H. DRIVE VEHICLES> A cable-type accelerator mechanical suspended-type pedal has been adopted.
<4G69-R.H. DRIVE VEHICLES> For the accelerator system, an electronic throttle actuator control system is utilized, eliminating the accelerator cable.

[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation