[27A] REAR AXLE <2WD> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION
The rear axle has the following features: The wheel bearing is a unit ball bearing (double-row angular contact ball bearing) which incorporates the oil seals and is highly resistant to a thrust load. ABS rotor for detecting the wheel speed is press-fitted to the rear hub in vehicles with ABS.
CONSTRUCTION DIAGRAM

[27A] REAR AXLE <2WD> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation